For 1990-2009 cars

## Rear Seat Armrest Replacement With 40 Percent Seat

Callout | Component Name
--- | ---
1 | Rear Seat Armrest Stop Cap
2 | Rear Seat Bolt Caution: Refer to Fastener Caution in the Preface section. Tighten 28 N·m (21 lb ft)
3 | Rear Seat Armrest Assembly

## Rear Seat Armrest Replacement With 60 Percent Seat

Callout | Component Name
--- | ---

#### Preliminary Procedures

Remove the rear seat back cushion outer cover. Refer to Rear Seat Back Cushion Cover Replacement.

1 | Rear Seat Armrest Bolt Caution: Refer to Fastener Caution in the Preface section. Tighten 10 N·m (89 lb in)
2 | Rear Seat Armrest