For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the rear seat No. 2 back cushion cover and pad. Refer to Rear Seat Number 2 Back Cushion Cover and Pad Replacement.
2. Remove the rear seat No. 2 cushion cover and pad. Refer to Rear Seat Number 2 Cushion Cover and Pad Replacement.

1 | Rear Seat No. 2 Recliner Inner Finish Cover Screw (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 5 N·m (44 lb in)
2 | Rear Seat No. 2 Recliner Inner Finish Cover (Qty: 2)