For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the steering column lower trim cover bolts. Refer to Steering Column Lower Trim Cover Replacement.

1 | Ignition Lock Cylinder Opening Trim Cover Bolt (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 2 N·m (18 lb in)
2 | Ignition Lock Cylinder Opening Trim Cover

#### Procedure

1. Unclip the ignition lock cylinder opening trim cover from steering column lower trim cover.
2. Separate the ignition lock cylinder opening trim cover from the steering column upper trim cover.