For 1990-2009 cars

### Removal Procedure

1. Pull the weatherstrip/run channel (1) from the window frame opening.
2. Carefully twist and pull downward on the weatherstrip run channel releasing it from the upper door frame.
3. Remove the weatherstrip/run channel from the door.

### Installation Procedure

Important: Install the weatherstrip/run channel by fitting both corners to the upper door frame and then pushing inward on the sides.

1. Install the weatherstrip/run channel (1) to the door.
2. Press the weatherstrip/run channel (1) into the window frame opening.