For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the bodyside trim panel. Refer to Quarter Lower Rear Trim Panel Replacement.
2. Disconnect the power liftgate actuator rod. Refer to Liftgate Actuator Rod Replacement.

1 | Liftgate Close Actuator Control Module

#### Procedure

1. Disconnect the electrical connector.
2. Cut the tie strap, if equipped.

2 | Liftgate Close Actuator Motor Control Module Bolt (Qty: 5) Caution: Refer to Fastener Caution in the Preface section. Tighten 9 N·m (80 lb in)
3 | Liftgate Close Actuator Control Module

#### Procedure

Reprogram liftgate module. Refer to Liftgate Calibration.