For 1990-2009 cars

Callout | Component Name
--- | ---
Important: The following procedure indicates servicing the left side of the vehicle. The right side of the vehicle is similar.

#### Preliminary Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the rear tire and wheel. Refer to Tire and Wheel Removal and Installation

1 | Rear Lateral Link

#### Procedure

1. Remove the upper control arm bolt. Refer to Upper Control Arm Replacement.
2. Remove the lower control arm bolt. Refer to Lower Control Arm Replacement.

Tip
Support the lower control arm with a jack stand.