For 1990-2009 cars

### Removal Procedure

1. Remove the fuel injector sight shield. Refer to Fuel Injector Sight Shield Replacement.
2. Remove as much power steering fluid from the remote power steering fluid reservoir as possible.
3. Place drain pans under the vehicle as needed.
4. Disconnect the power steering fluid reservoir outlet hose (1) from the remote power steering fluid reservoir.
5. Disconnect the power steering fluid reservoir outlet hose (1) from the power steering pump.

Note: Disconnect any clips as needed before attempting removal.

6. Remove the power steering fluid reservoir outlet hose from the vehicle.

### Installation Procedure

Note: Clip the power steering fluid reservoir hose in place in its original routing.

1. Install the power steering fluid reservoir outlet hose to the vehicle.
2. Connect the power steering fluid reservoir outlet hose (1) to the power steering pump.
3. Connect the power steering fluid reservoir outlet hose (1) to the remote power steering fluid reservoir.
4. Clean all excess fluid from the vehicle and remove the drain pans.
5. Fill and bleed the power steering system. Refer to Power Steering System Bleeding.
6. Install the fuel injector sight shield. Refer to Fuel Injector Sight Shield Replacement.