For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove the seat back cushion cover and pad. Refer to Front Seat Back Cushion Cover and Cushion Pad Replacement.
2. Remove the front seat lumbar control. Refer to Front Seat Lumbar Control Replacement.

1 | Front Seat Lumbar Assembly Bolt (Qty: 4) Caution: Refer to Fastener Caution in the Preface section. Tighten 9 N·m (80 lb in)
2 | Front Seat Lumbar Assembly