For 1990-2009 cars

Callout | Component Name
--- | ---
Note: The following service procedure indicates the left side of the vehicle. The right side of the vehicle is similar.

#### Preliminary Procedure

Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.

1 | Stabilizer Shaft Clamp Bolt (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 50 N·m (37 lb ft)
2 | Stabilizer Shaft Clamp
3 | Stabilizer Shaft Insulator