For 1990-2009 cars

Table 1: | 4-5-6 Clutch Piston Installation
Table 2: | 4-5-6 Clutch Dam Installation
Table 3: | 4-5-6 Clutch Plates Installation
Table 4: | 3-5 Reverse Clutch Plates Installation
Table 5: | Piston and Reluctor Wheel Installation
Table 6: | 3-5-R and 4-5-6 Clutch Piston Air Check

### 4-5-6 Clutch Piston Installation

Callout | Component Name
--- | ---
1 | 4-5-6 Clutch Piston Inner Seal
2 | 4-5-6 Clutch Piston Outer Seal (Rounded)
3 | 4-5-6 Clutch Piston Outer Seal (Stepped) (Orange)
4 | 4-5-6 Clutch Piston Tip DT-47859 outer seal protector prevents the piston seal lip from damage during installation. Apply a thin coat of ATF to the I.D. of DT-47859 outer seal protector to ease the installation of the piston.

#### Special Tools

DT-47859 Piston Outer Seal Protector

For equivalent regional tools, refer to Special Tools.

### 4-5-6 Clutch Dam Installation

Callout | Component Name
--- | ---
1 | 4-5-6 Clutch Spring
2 | 4-5-6 Clutch Piston Fluid Dam Tip DT 47693-1 which is part of DT-47693 dam protector prevents the dam seal lip from damage during installation. Apply a thin coat of ATF to the I.D. of DT 47693-1 which is part of DT-47693 dam protector to ease the installation of the dam.

#### Special Tools

DT-47693 Dam Protector

For equivalent regional tools, refer to Special Tools.

3 | 4-5-6 Clutch Dam Retaining Ring

#### Special Tools

• | DT 47693-2 Clutch Spring Compressor which is part of DT-47693 dam protector

• | J 8059 Snap Ring Pliers-Parrallel Jaw or equivalent

For equivalent regional tools, refer to Special Tools.

### 4-5-6 Clutch Plates Installation

Callout | Component Name
--- | ---
1 | 4-5-6 Clutch Hub Thrust Bearing Tip Note location of the orientation lip on bearing. All thrust bearings can only be assembled one way.
2 | Reaction Carrier Hub Assembly Caution: Failure to use DT 48551 could cause damage to the hub assembly bushings which could cause premature transmission failure.

#### Special Tools

DT-48551 Reaction Hub Bushing Protector

For equivalent regional tools, refer to Special Tools.

3 | 4-5-6 Clutch Plate (Qty: 6)
4 | 4-5-6 Clutch (w/Friction Material) Plate Assembly (Qty: 6)
5 | 4-5-6 Clutch Backing Plate
6 | 4-5-6 Clutch Backing Plate Retaining Ring Tip Gently push down on the backing plate to get enough clearance between the backing plate and retainer.

### 3-5 Reverse Clutch Plates Installation

Callout | Component Name
--- | ---
1 | 3-5 Reverse Clutch (Waved) Plate
2 | 3-5 Reverse Clutch Plate (Qty: 4)
3 | 3-5 Reverse Clutch (w/Friction Material) Plate Assembly (Qty: 4)
4 | 3-5 Reverse Clutch Backing Plate
5 | 3-5 Reverse Clutch Backing Plate Retaining Ring

### Piston and Reluctor Wheel Installation

Callout | Component Name
--- | ---
1 | 3-5 Reverse Clutch Piston Dam Seal
2 | 3-5 Reverse Clutch Piston Inner Seal (Black) Tip Apply a thin coat of ATF to the seal to ease the installation of the piston.
3 | 3-5 Reverse Clutch Piston Inner Seal (Orange) Tip Apply a thin coat of ATF to the seal to ease the installation of the piston.
4 | 3-5 Reverse Clutch Spring Assembly
5 | 3-5 Reverse Clutch Piston Tip

• | J-46622 seal protector prevents the piston seal lip from damage during installation. Apply a thin coat of ATF to the I.D. of J-46622 seal protector to ease the installation of the piston.

• | Install J-46622 seal protector onto the speed sensor reluctor wheel. Push the 3-5 Reverse Clutch piston into the reluctor wheel until it stops against J-46622 seal protector . Remove J-46622 seal protector by separating it at the opening.

#### Special Tools

J-46622 Piston Seal Protector

For equivalent regional tools, refer to Special Tools.

6 | A/Trans Input Shaft Speed Sensor Reluctor Wheel
7 | A/Trans Input Shaft Speed Sensor Reluctor Wheel Retaining Ring Caution: Compress the reluctor wheel just enough to clear the retainer ring groove. Over compressing the reluctor wheel will break the alignment tab and the clutch housing.

#### Special Tools

DT-47694 Piston Spring Compressor

For equivalent regional tools, refer to Special Tools.

### 3-5-R and 4-5-6 Clutch Piston Air Check

Callout | Component Name
--- | ---
1 | Case Cover Assembly Tip The fluid seal rings should be in place and not damaged.
2 | Apply shop air to the 4-5-6 clutch feed. Observe the 4-5-6 piston movement. Caution: Regulate the air pressure to 40 psi maximum. High pressure could cause the piston to over travel and damage the piston seals. Tip Minimal piston movement and excessive air leaking could indicate damage to the 4-5-6 piston seals or improper assembly.
3 | Apply shop air to the 3-5-Rev clutch feed. Observe the 3-5-Rev piston movement. Caution: Regulate the air pressure to 40 psi maximum. High pressure could cause the piston to over travel and damage the piston seals. Tip Minimal piston movement and excessive air leaking could indicate damage to the 3-5-Rev piston seals or improper assembly.