For 1990-2009 cars

## Video Display Replacement U42

Callout | Component Name
--- | ---
1 | Video Display Assembly Screw (Qty: 4) Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

Make sure that all 4 washers on the 4 mounting screws are accounted for. If any washers are off the screw and loose, discard to prevent a rattle. The washers were required only for assembly plant installation, and can be used if still on the screw or they can be discarded.

Tighten
2 N·m (18 lb in)

2 | Video Display Assembly

#### Procedure

1. Pull down to disengage the retainer clip and remove from the vehicle.
2. Disconnect the electrical connector.

## Video Display Replacement U42/C3U

Callout | Component Name
--- | ---
1 | Video Display Assembly Screw (Qty: 4) Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

Make sure that all 4 washers on the 4 mounting screws are accounted for. If any washers are off the screw and loose, discard to prevent a rattle. The washers were required only for assembly plant installation, and can be used if still on the screw or they can be discarded.

Tighten
2 N·m (18 lb in)

2 | Video Display Assembly

#### Procedure

1. Pull down to disengage the retainer clip and remove from the vehicle.
2. Disconnect the electrical connector.