For 1990-2009 cars

### Removal Procedure

1. Open the door.
2. Remove the door trim panel. Refer to Rear Side Door Trim Panel Replacement .
3. Remove the retainer (1).
4. Carefully remove the water deflector from the door by releasing the adhesive backing.

### Installation Procedure

1. Position the water deflector to the door.
2. Install the retainers (1).
3. Press the water deflector to the door. Ensure that the water deflector forms a proper seal around the surface of the door panel.
4. Install the door trim panel. Refer to Rear Side Door Trim Panel Replacement .