For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Hood Rear Outer Seal

#### Procedure

1. Clean the area where the seal will be mounted. Use a suitable solvent with a mixture of 50 percent isopropyl alcohol and 50 percent water by volume, or high-flash naphtha.
2. Warm the hood panel using J 25070 Heat Gun, to a minimum, prior to the hood rear outer seal installation.
3. Do NOT touch the adhesive surface when tape is removed. Peel the tape liner off and install the outer rear hood seal.

#### Special Tools

J 25070 Heat Gun