For 1990-2009 cars

## Front Wheel Drive Shaft Seal Replacement - Right Side Front Wheel Drive

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Raise the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Remove the intermediate drive shaft. Refer to Intermediate Drive Shaft Replacement .

1 | Right Front Wheel Drive Shaft Oil Seal Tip

• | For seal removal use J 6125-1B Slide Hammer with J 23129 Universal Seal Remover.

• | For seal installation use J 8092 Driver Handle with J-46629-A Axle Seal Installer. The axle seal installer has no depth stop, be careful to NOT install the seal too deep, ensure the seal is installed flush and level with the transmission case surface for proper sealing.

#### Special Tools

• | J 8092 Driver Handle

• | J-46629-A Axle Seal Installer