For 1990-2009 cars

#### Special Tools

• | EN-46106 Engine Flywheel Holding Tool

• | J-41998-B Crankshaft Balancer Installer

• | J-45059 Angle Meter

| For equivalent regional tools, refer to Special Tools.

1. The EN-46106 tool must be installed onto the flywheel.
2. Use the J-41998-B installer , nut, bearing and washer to install the crankshaft balancer.

Note: Do not lubricate the crankshaft front oil seal or crankshaft balancer sealing surfaces. The crankshaft balancer is installed into a dry seal.

3. Apply lubricant to the inside of the crankshaft balancer hub bore.
4. Place the crankshaft balancer in position on the crankshaft.
5. Thread the J-41998-B installer in the crankshaft. Ensure you engage at least 10 threads of the J-41998-B installer before pressing the crankshaft balancer in place.
6. Push the crankshaft balancer into position by tightening the nut on the J-41998-B installer until the large washer bottoms out on the crankshaft end.
7. Remove the J-41998-B installer .
8. Install the crankshaft balancer bolt.

Caution: Refer to Fastener Caution in the Preface section.

9. Tighten the crankshaft balancer bolt to 100 N·m (74 lb ft) and an additional 150 degrees using the J-45059 meter .
10. Remove the EN-46106 tool .