For 1990-2009 cars

## Rear Seat Recliner Outer Finish Cover Replacement - Inboard with 40 Percent Seat

Callout | Component Name
--- | ---
1 | Rear Seat Recliner Outer Finish Cover

#### Procedure

1. Move the seat forward to the Smart Slide® E-Z entry position.
2. Remove the rear seat recliner outer finish cover by pulling outward to disengage the retainers.
3. When reinstalling the cover, ensure that the inboard recliner cable is above the push-in retainer.

2 | Push-in Retainer
3 | Retainer Clip (Qty: 2)