For 1990-2009 cars

#### Special tools

J 35910 Drive Axle Seal Clamp Pliers

### Disassemble Procedure

1. Remove the wheel drive shaft from the vehicle. Refer to Front Wheel Drive Shaft Replacement.
2. Install the wheel drive shaft in a soft jawed vise.
3. Using a pair of side cutters, remove and discard the small boot clamp (4) from the boot (3).
4. Using the appropriate tool, remove and discard the large boot clamp (2) from the boot (3).
5. Remove the boot (3) from the from the tripot housing (1).
6. Remove the inner tripot housing (1) from the wheel drive shaft (3).
7. Using the appropriate tool, remove the outer tripot spider retaining ring (1) from the wheel drive shaft (5).
8. Remove the tripot spider (2) from the wheel drive shaft (5).

Note: Step 9 is for those vehicles that have an inner retaining ring for the tripot spider. If there isn't an inner retaining ring, skip step 9 and proceed to step 10.

9. Using the appropriate tool, remove the inner tripot retaining ring (3), if equipped, from the wheel drive shaft (5).
10. Remove the wheel drive shaft boot (4) from the wheel drive shaft (5).
11. Inspect the wheel drive shaft inner joint. Refer to Wheel Drive Shaft Inner Joint Inspection.

### Assemble Procedure

1. Install the boot (1) on the wheel drive shaft (3).
2. Ensure that the boot (1) is properly seated in the groove (2) in the wheel drive shaft.

Note: Step 3 is for those vehicles that have an inner retaining ring for the tripot spider. If there isn't an inner retaining ring, skip step 3 and proceed to step 4.

3. Using the appropriate tool, install the inner tripot retaining ring (3), if equipped.
4. Install the tripot spider (2) until just touches the shoulder on the wheel drive shaft (5).
5. Using the appropriate tool, install the outer tripot spider retaining ring (1).
6. Using the J 35910 Drive Axle Seal Clamp Pliers (1), close the boot clamp (2) until the gap (3) measures 1.8 mm (0.07 inch).
7. Install the tripot housing (1) on the wheel drive shaft (3).
8. Install the wheel drive shaft boot (3) on the tripot housing (1).
9. Place approximately half of the lubricant (2) in the boot (1) and the remaining half in the tripot housing (3).
10. Using the J 35910 Drive Axle Seal Clamp Pliers (3), ratchet wrench (4) and a breaker bar (5), close the boot clamp (1) until the gap (6) measures 1.9 mm (0.07 inch).
11. Remove any of the excess lubricant from the tripot housing and wheel drive shaft.
12. Move the tripot joint housing in a circular motion to distribute the lubricant in the tripot housing.
13. Remove the wheel drive shaft from the vise.
14. Install the wheel drive shaft in the vehicle. Refer to Front Wheel Drive Shaft Replacement.