For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Disconnect the battery. Refer to Battery Negative Cable Disconnection and Connection .
2. Remove the junction block cover.

1 | Battery Positive Cable to Junction Block Nut

#### Procedure

Disconnect the battery positive cable from the junction block by removing the nut.

2 | Junction Block Bolt (Qty: 2)

#### Procedure

Turn the bolt until an audible sound is heard and ENSURE the location of tabs are drawn up flush with the fuse center top surface.

3 | Underhood Electrical Center or Junction Block

#### Procedure

1. Upon installation of the upper fuse box, ensure the 2 orange indicators are visible to have a proper installation of the lower connector to the upper fuse box.
2. Use a hook-like tool to disengage the 7 tabs.
3. Disconnect any electrical connectors
4. Transfer components as necessary.