For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the rear seat track covers. Refer to Rear Seat Track Front Inboard Cover, Front Outboard Cover, Rear Inboard Cover, and Rear Outboard Cover Replacement.

1 | Rear Floor Console Bolt (Qty: 4) Caution: Refer to Fastener Caution in the Preface section. Tighten 45 N·m (33 lb ft)
2 | Rear Floor Console Assembly

#### Procedure

1. Disconnect the electrical connections.
2. When replacing the rear floor console assembly, transfer all necessary components.