For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Accelerator Pedal Position (APP) Sensor Bolt | 8 N·m | 71 lb in
Air Cleaner Lower Housing Screw | 9 N·m | 80 lb in
Air Cleaner Outlet Duct Clamp | 4 N·m | 35 lb in
Camshaft Position (CMP) Actuator Solenoid Valve Bolt | 10 N·m | 89 lb in
Camshaft Position (CMP) Sensor Bolt | 10 N·m | 89 lb in
Crankshaft Position (CKP) Sensor Bolt | 10 N·m | 89 lb in
Engine Control Module (ECM) Bracket Bolt | 6 N·m | 53 lb in
Engine Coolant Temperature (ECT) Sensor | 22 N·m | 16 lb ft
Evaporative Emission (EVAP) Purge Solenoid Valve Bracket Bolt | 10 N·m | 89 lb in
Fuel Feed/Evaporative Emission (EVAP) Pipe Clip Bolt | 8 N·m | 71 lb in
Fuel Feed/Evaporative Emission (EVAP) Pipe Clip Nut | 9 N·m | 80 lb in
Fuel Rail Bolt | 10 N·m | 89 lb in
Fuel Tank Fill Hose Clamp | 3.3 N·m | 29 lb in
Fuel Tank Fill Pipe Bracket Bolt | 12 N·m | 106 lb in
Fuel Tank Fill Pipe Housing to Fuel Tank Fill Pipe Bolt | 2 N·m | 18 lb in
Fuel Tank Strap Bolt | 47 N·m | 35 lb ft
Heated Oxygen Sensor (HO2S) | 42 N·m | 31 lb ft
Intake Manifold Tuning Valve Bolt | 10 N·m | 89 lb in
Ignition Coil Bolt | 10 N·m | 89 lb in
Knock Sensor Bolt | 23 N·m | 17 lb ft
Mass Air Flow (MAF)/Intake Air Temperature Sensor Screw | 4 N·m | 35 lb in
Manifold Absolute Pressure (MAP) Sensor Bolt | 10 N·m | 89 lb in
Power Steering Fluid Reservoir Bracket Bolt | 9 N·m | 80 lb in
Spark Plug | 20 N·m | 15 lb ft
Throttle Body Bolt | 10 N·m | 89 lb in
Underhood Bussed Electrical Center (UBEC) Bracket Bolt/Nut | 10 N·m | 89 lb in