For 1990-2009 cars

### Removal Procedure

1. Starting at the bottom of the sealing strip, pull the sealing strip away from the door pinch-weld flange.
2. Lift upward in order to remove the upper portion of the sealing strip from the door pinch-weld flange.
3. Remove the sealing strip from the door.

### Installation Procedure

1. Starting at the top of the sealing strip, insert the sealing strip tab into the door sheet metal.
2. Position the sealing strip to the door pinch-weld flange and apply pressure in order to seat the sealing strip.
3. Ensure that the sealing strip is fully seated against the pinch-weld flange.