For 1990-2009 cars

## Rocker Panel Rear Molding Replacement Traverse

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Open the rear door in order to remove the rocker panel rear molding.
2. Release the front and rear side door weatherstrip retainer from the rear rocker panel molding.

1 | Rear Rocker Panel Screw (Qty: 3) Caution: Refer to Fastener Caution in the Preface section. Tighten 1.5 N·m (13 lb in)
2 | Rocker Panel Molding W-clip (Qty: 3)
3 | Rocker Panel Rear Molding Assembly

#### Procedure

1. Release the three retainers from the back side of the molding and remove.
2. Slide the rear rocker panel molding from the rear edge of the front rocker panel molding.

## Rocker Panel Rear Molding Replacement Acadia

Callout | Component Name
--- | ---

#### Preliminary Procedure

Open the rear door in order to remove the rocker panel rear molding.

1 | Rear Rocker Panel Finish Panel Screw (Qty: 3) Caution: Refer to Fastener Caution in the Preface section. Tighten 1.5 N·m (13 lb in)
2 | Rocker Panel Molding Retainers (Qty: 2)
3 | Rocker Panel Rear Molding Assembly

#### Procedure

Release the 2 retainers from the back side of the molding and remove.

## Rocker Panel Rear Molding Replacement OUTLOOK

Callout | Component Name
--- | ---

#### Preliminary Procedure

Open the rear door in order to remove the rocker panel rear molding.

1 | Rear Rocker Panel Finish Panel Screw (Qty: 3) Caution: Refer to Fastener Caution in the Preface section. Tighten 1.5 N·m (13 lb in)
2 | Rocker Panel Rear Molding Assembly Tip Release the 2 retainers from the back side of the molding and remove.