For 1990-2009 cars

1. Position a NEW oil filter adapter gasket onto the oil filter adapter.
2. Place the oil filter adapter into position.

Caution: Refer to Fastener Caution in the Preface section.

3. Install the oil filter adapter bolts. Ensure the longer bolts (1) is installed in the upper rear position and tighten the oil filter adapter bolts to 23 N·m (17 lb ft).
4. Install a NEW oil filter.