For 1990-2009 cars

## Front Bumper Fascia Replacement Traverse

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the front compartment sight shield. Refer to Front Compartment Sight Shields Replacement.
2. Remove the front wheelhouse front liner. Refer to Front Wheelhouse Front Liner Replacement.

1 | Front Bumper Fascia Push-Pin (Qty: 4)
2 | Front Bumper Fascia Screw (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 10 N·m (89 lb in)
3 | Front Bumper Fascia Fender Tab Tip Carefully push a small nylon wedge between the fascia and the fender. Insert a small flat-bladed tool into the fascia slot and depress the tabs one at a time and pull on the fascia at the same time to gradually remove the fascia from the fender.
4 | Front Bumper Fascia Headlamp Bracket Tip Carefully push a small nylon wedge between the fascia and the fender. Insert a small flat-bladed tool into the fascia slot and depress the tabs one at a time and pull on the fascia at the same time to gradually remove the fascia from the headlamp bracket.
5 | Front Bumper Fascia

#### Procedure

• | Disconnect any electrical connectors.

• | Transfer parts as needed.

## Front Bumper Fascia Replacement Acadia

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the front compartment sight shields. Refer to Front Compartment Sight Shields Replacement.
2. Remove the front wheelhouse liner. Refer to Front Wheelhouse Front Liner Replacement.

1 | Front Fascia Screw (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tip Reach underneath the wheelhouse to access the bolts. Tighten
2 N·m (18 lb in)

2 | Front Fascia Retainer (Qty: 6)
3 | Front Fascia Bracket Screw (Qty: 2) Tighten 2 N·m (18 lb in)
4 | Front Fascia

#### Procedure

1. Drill out the license plate bracket rivets, if equipped.
2. Disconnect any electrical connectors.
3. Transfer parts as needed.
4. Pull forward to remove the front bumper fascia.

## Front Bumper Fascia Replacement Enclave

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the front compartment sight shield. Refer to Front Compartment Sight Shields Replacement.
3. Remove the front wheelhouse liner. Refer to Front Wheelhouse Front Liner Replacement.

1 | Front Fascia Bolt (Qty: 16) Caution: Refer to Fastener Caution in the Preface section. Tighten 2 N·m (18 lb in)
2 | Front Fascia Retainer (Qty: 4)
3 | Front Fascia

#### Procedure

1. Drill out the license plate bracket rivets, if equipped.
2. Disconnect any electrical connectors.
3. Transfer components as necessary.
4. Pull forward to remove the front bumper fascia.

## Front Bumper Fascia Replacement OUTLOOK

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the front compartment sight shields. Refer to Front Compartment Sight Shields Replacement.
2. Remove the front wheelhouse liner. Refer to Front Wheelhouse Front Liner Replacement.

1 | Front Fascia Screw (Qty: 3) Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

Reach underneath the fender to access the bolts.

Tighten
2 N·m (18 lb in)

2 | Front Fascia Retainer (Qty: 4)
3 | Front Fascia Bracket Screw (Qty: 2) Tighten 2 N·m (18 lb in)
4 | Front Fascia

#### Procedure

1. Drill out the license plate bracket rivets, if equipped.
2. Disconnect any electrical connectors.
3. Transfer parts as needed.
4. Pull forward to remove the front bumper fascia.