For 1990-2009 cars

Table 1: | Reluctor Wheel and Piston Removal
Table 2: | Clutch Plate Removal
Table 3: | 4-5-6 Clutch Hub Removal
Table 4: | 4-5-6 Clutch Piston Removal

### Reluctor Wheel and Piston Removal

Callout | Component Name
--- | ---
1 | A/Trans Input Shaft Speed Sensor Reluctor Ring Retaining Ring Caution: Compress the reluctor wheel just enough to clear the retainer. Over compressing the reluctor wheel will break the alignment tab and the clutch housing.

#### Special Tools

DT-47694 Piston Spring Compressor

For equivalent regional tools, refer to Special Tools.

2 | A/Trans Input Shaft Speed Sensor Reluctor Wheel
3 | 3-5 Reverse Clutch Piston Tip Inspect piston seals for damage and/or wear. Piston is reusable.
4 | 3-5 Reverse Clutch Spring Assembly
5 | 3-5 Reverse Clutch Piston Inner Seal (Orange)
6 | 3-5 Reverse Clutch Piston Inner Seal (Black)
7 | 3-5 Reverse Clutch Piston Dam Seal

### Clutch Plate Removal

Callout | Component Name
--- | ---
1 | 3-5 Reverse Clutch Backing Plate Retaining Ring
2 | 3-5 Reverse Clutch Backing Plate
3 | 3-5 Reverse Clutch (w/Friction Material) Plate Assembly (Qty: 4)
4 | 3-5 Reverse Clutch Plate (Qty: 4)
5 | 3-5 Reverse Clutch (Waved) Plate

### 4-5-6 Clutch Hub Removal

Callout | Component Name
--- | ---
1 | 4-5-6 Backing Plate Retaining Ring Tip Gently push down on the backing plate to get enough clearance between the backing plate and retainer.
2 | Reaction Carrier Hub Assembly Tip The clutch plates will come out of the housing with the hub assembly.
3 | 4-5-6 Clutch Backing Plate
4 | 4-5-6 Clutch Plate (Qty: 6)
5 | 4-5-6 Clutch (w/Friction Material) Plate Assembly (Qty: 6)
6 | 4-5-6 Clutch Hub Thrust Bearing Assembly Tip The bearing may stick to the reaction carrier hub.

### 4-5-6 Clutch Piston Removal

Callout | Component Name
--- | ---
1 | 4-5-6 Clutch Dam Retaining Ring

#### Special Tools

• | DT-47693 Dam Protector

• | J 8059 Snap Ring Pliers-Parallel Jaw or equivalent

For equivalent regional tools, refer to Special Tools.

2 | 4-5-6 Clutch Piston Fluid Dam

#### Procedure:

1. Place the 3-5-R and 4-5-6 clutch housing onto the case cover assembly.
2. Apply shop air to the 4-5-6 clutch feed hole using a rubber tipped air gun to dislodge the dam piston and the 4-5-6 clutch piston from the clutch housing.

3 | 4-5-6 Clutch Spring Assembly
4 | 4-5-6 Clutch Piston
5 | 4-5-6 Clutch Piston Outer Seal (Stepped)
6 | 4-5-6 Clutch Piston Outer Seal (Rounded)
7 | 4-5-6 Clutch Piston Inner Seal