For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the interior trim panel. Refer to Rear Side Door Trim Panel Replacement.
2. Remove the water deflector. Refer to Rear Side Door Water Deflector Replacement.
3. Rear the rear door energy absorber pad. Rear Door Energy Absorber Pad Replacement.

1 | Rear Side Door Lock Bolt (Qty: 2) Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

Remove the rear lower section of the run channel only.

Tighten
10 N·m (89 lb in)

2 | Rear Side Door Lock Assembly

#### Procedure

1. Release the inside handle cable retainers before removing the door lock.
2. Disconnect the door lock electrical connector.
3. Transfer the lock rods.