For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

Remove front door trim panel. Refer to Front Side Door Trim Panel Replacement - Left Side or Front Side Door Trim Panel Replacement - Right Side .

1 | Front Side Door Inner Window Sealing Strip

#### Procedure

1. Start from the front edge of the door, pull upward on the inner window sealing strip to release it from the pinch-weld flange.
2. Install the inner window sealing strip to the front edge of the door, press firmly onto the pinch-weld flange and work it rearward.