For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Disable the SIR system. Refer to SIR Disabling and Enabling.
2. Remover center pillar upper molding. Refer to Center Pillar Upper Garnish Molding Replacement.
3. Remove front seat belt. Refer to Seat Belt Retractor Pretensioner Replacement - Front.

1 | Front Seat Shoulder Belt Guide Adjuster Bolt (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 50 N·m (37 lb ft)
2 | Front Seat Shoulder Belt Guide Adjuster Assembly