For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the bumper fascia. Refer to Rear Bumper Fascia Replacement.

1 | Rear Bumper Impact Bar Bracket Bolt (Qty: 6) Caution: Refer to Fastener Caution in the Preface section. Tighten 30 N·m (22 lb ft)
2 | Rear Bumper Impact Bar

#### Procedure

1. Unclip the electrical harness from the impact bar.
2. Transfer the necessary components.