For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Raise the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Remove the left wheel drive shaft. Refer to Front Wheel Drive Shaft Replacement .

1 | Left Front Wheel Drive Shaft Oil Seal

#### Procedure

• | For seal removal use J 6125-1B Slide Hammer with J 23129 Universal Seal Remover.

• | For seal installation use J 8092 Driver Handle with J-46629-A Axle Seal Installer. The axle seal installer has no depth stop, be careful to NOT install the seal too deep, ensure the seal is installed flush and level with the transmission case surface for proper sealing.

#### Special Tools

• | J 8092 Driver Handle

• | J-46629-A Axle Seal Installer