For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the instrument panel trim pad. Refer to Instrument Panel Trim Pad Replacement.

1 | Instrument Panel Inflatable Restraint Module Nut (Qty: 4) Caution: Refer to Fastener Caution in the Preface section. Tighten 10 N·m (89 lb in)
2 | Instrument Panel Inflatable Restraint Module

#### Procedure

Fully deploy the module before disposal. If the module was replaced under warranty, fully deploy and dispose of the module, after the required retention period. Refer to Inflator Module Handling and Scrapping.