For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the rear floor console rear trim lower panel Assembly. Refer to Rear Floor Console Rear Trim Lower Panel Replacement.
2. Remove the rear floor console front trim panel assembly - Lower. Refer to Rear Floor Console Front Trim Panel Replacement.
3. Remove the rear floor console front trim upper panel assembly. Refer to Rear Floor Console Front Trim Upper Panel Replacement.

1 | Rear Floor Console Side Trim Panel Screw (Qty: 4) Caution: Refer to Fastener Caution in the Preface section. Tighten 2.5 N·m (22 lb in)
2 | Rear Floor Console Side Trim Panel Assembly

#### Procedure

Grasp the trim panel and pull outward in order to release the clips securing the side trim panel to the console assembly.