For 1990-2009 cars

## Front Air Deflector Replacement Acadia

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the front bumper fascia bracket. Refer to Front Bumper Fascia Bracket Replacement .

1 | Front Bumper Air Deflector Plastic Retainers (Qty: 15)
2 | Front Bumper Fascia Extension

## Front Air Deflector Replacement Traverse

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the front wheelhouse front liner. Refer to Front Wheelhouse Front Liner Replacement.

1 | Front Bumper Air Deflector Plastic Retainer (Qty: 14)
2 | Front Bumper Air Deflector

#### Procedure

Remove the deflector pulling forward to release the retainer tabs.

## Front Air Deflector Replacement Enclave

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the Parking and Front Fog Lamp Bracket. Refer to Parking and Front Fog Lamp Bracket Replacement.
2. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.

1 | Front Bumper Air Deflector Bolts (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 2 mm N·m (0.79 lb in)
2 | Front Bumper Fascia Air Deflector

## Front Air Deflector Replacement OUTLOOK

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the front wheelhouse front liner. Refer to Front Wheelhouse Front Liner Replacement.

1 | Front Bumper Lower Fascia Bolt (Qty: 16) Caution: Refer to Fastener Caution in the Preface section. Tighten 6 N·m (53 lb in)
2 | Front Bumper Air Deflector Plastic Retainer (Qty: 16)
3 | Front Bumper Air Deflector

#### Procedure

Remove the deflector pulling forward to release the retainer tabs.