For 1990-2009 cars

### Removal Procedure

1. Remove the fuel injector sight shield. Refer to Fuel Injector Sight Shield Replacement.
2. Remove as much power steering fluid from the remote power steering fluid reservoir as possible.
3. Place drain pans under the vehicle as needed.
4. Compress the power steering reservoir inlet hose clamp (1) and disconnect the hose from the remote power steering fluid reservoir.
5. Compress the power steering fluid reservoir outlet hose clamp (1) and disconnect the hose from the remote power steering fluid reservoir.
6. Remove the remote power steering fluid reservoir bolts (1).
7. Remove the remote power steering fluid reservoir (2).

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the remote power steering fluid reservoir (2).
2. Install the remote power steering fluid reservoir bolts (1) and tighten to 9 N·m (80 lb in).
3. Connect the power steering fluid reservoir outlet hose and clamp (1).
4. Connect the power steering reservoir inlet hose and clamp (1).
5. Clean all excess fluid from the vehicle and remove the drain pans.
6. Fill and bleed the power steering system. Refer to Power Steering System Bleeding.
7. Install the fuel injector sight shield. Refer to Fuel Injector Sight Shield Replacement.