For 1990-2009 cars

Table 1: | Memory Seat Module Scan Tool Data Parameters
Table 2: | Memory Seat Module Scan Tool Output Controls

#### Memory Seat Module Scan Tool Data Parameters

Parameter | System State | Expected Value | Definition
--- | --- | --- | ---
Operating Conditions: Ignition ON
Driver Seat Front Vertical Sensor | -- | Varies | This displays Volts. This is the voltage supplied to the driver seat front vertical sensor.
Driver Seat Horizontal Sensor | -- | Varies | This displays Volts. This is the voltage supplied to the driver seat horizontal sensor.
Driver Seat HVC Level | -- | High | The scan tool displays High, Medium or Low. This is the current level of the driver heated seat or the heated cooled seat.
Driver Seat HVC Mode | -- | Off | The scan tool displays Off, Back & Cushion, Back Only or Cool. This is the current mode of the driver heated seat or the heated cooled seat.
Driver Seat Rear Vertical Sensor | -- | Varies | This displays Volts. This is the voltage supplied to the driver seat rear vertical sensor.
Driver Seat Recline Sensor | -- | Varies | This displays Volts. This is the voltage supplied to the driver seat recline sensor.
Front Vertical Downward Switch | -- | Inactive | The scan tool displays Active or Inactive. This is the state of the front vertical downward switch.
Front Vertical Motor Downward | -- | Inactive | The scan tool displays Active or Inactive. This is the state of the front vertical motor downward.
Front Vertical Motor Upward | -- | Inactive | The scan tool displays Active or Inactive. This is the state of the front vertical motor upward.
Front Vertical Upward Switch | -- | Inactive | The scan tool displays Active or Inactive. This is the state of the front vertical upward switch.
Horizontal Forward Switch | -- | Inactive | The scan tool displays Active or Inactive. This is the state of the horizontal forward switch.
Horizontal Motor Forward | -- | Inactive | The scan tool displays Active or Inactive. This is the state of the horizontal motor forward.
Horizontal Motor Rearward | -- | Inactive | The scan tool displays Active or Inactive. This is the state of the horizontal motor rearward.
Horizontal Rearward Switch | -- | Inactive | The scan tool displays Active or Inactive. This is the state of the horizontal rearward switch.
Lumbar Downward Switch | -- | Inactive | The scan tool displays Active or Inactive. This is the state of the lumbar downward switch.
Lumbar Forward Switch | -- | Inactive | The scan tool displays Active or Inactive. This is the state of the lumbar forward switch.
Lumbar Horizontal Sensor | -- | Varies | This displays Volts. This is the voltage supplied to the lumbar horizontal sensor.
Lumbar Inflation Value | -- | Varies | This displays Volts. This is the voltage stored in memory for the lumbar inflation.
Lumbar Vertical Sensor | -- | Varies | This displays Volts. This is the voltage supplied to the lumbar vertical sensor.
Lumbar Motor Downward | -- | Inactive | The scan tool displays Active or Inactive. This is the state of the lumbar motor downward.
Lumbar Motor Forward | -- | Inactive | The scan tool displays Active or Inactive. This is the state of the lumbar motor forward.
Lumbar Motor Rearward | -- | Inactive | The scan tool displays Active or Inactive. This is the state of the lumbar motor rearward.
Lumbar Motor Upward | -- | Inactive | The scan tool displays Active or Inactive. This is the state of the lumbar motor upward.
Lumbar Rearward Switch | -- | Inactive | The scan tool displays Active or Inactive. This is the state of the lumbar rearward switch.
Lumbar Upward Switch | -- | Inactive | The scan tool displays Active or Inactive. This is the state of the lumbar upward switch.
Lumbar Vertical Position | -- | Varies | This displays Volts. This is the voltage stored in memory for the lumbar vertical position.
Lumbar Vertical Sensor | -- | Varies | This displays Volts. This is the voltage supplied to the lumbar vertical sensor.
Massage Switch | -- | Inactive | The scan tool displays Active or Inactive. This is the state of the massage switch.
Lumbar Vertical Position | -- | Varies | This displays Volts. This is the voltage stored in memory for the lumbar vertical position.
Memory 1 Adj. Pedals Position | -- | Varies | This displays Volts. This is the voltage stored in memory for the position of the adjustable pedals.
Memory 2 Adj. Pedals Position | -- | Varies | This displays Volts. This is the voltage stored in memory for the position of the adjustable pedals.
Passenger Seat HVC Mode | -- | Off | The scan tool displays Off, Back & Cushion, Back Only or Cool. This is the current mode of the passenger heated seat or the heated cooled seat.
Rear Vertical Downward Switch | -- | Inactive | The scan tool displays Active or Inactive. This is the state of the rear vertical downward switch.
Rear Vertical Motor Downward | -- | Inactive | The scan tool displays Active or Inactive. This is the state of the rear vertical motor downward.
Rear Vertical Motor Upward | -- | Inactive | The scan tool displays Active or Inactive. This is the state of the rear vertical motor upward.
Rear Vertical Upward Switch | -- | Inactive | The scan tool displays Active or Inactive. This is the state of the rear vertical upward switch.
Recline Forward Switch | -- | Inactive | The scan tool displays Active or Inactive. This is the state of the recline forward switch.
Recline Motor Forward | -- | Inactive | The scan tool displays Active or Inactive. This is the state of the recline motor forward.
Recline Motor Rearward | -- | Inactive | The scan tool displays Active or Inactive. This is the state of the recline motor rearward.
Recline Rearward Switch | -- | Inactive | The scan tool displays Active or Inactive. This is the state of the recline rearward switch.
Seat Front Vertical Position | -- | Varies | This displays Volts. This is the voltage stored in memory for the seat front vertical position.
Seat Horizontal Position | -- | Varies | This displays Volts. This is the voltage stored in memory for the seat horizontal position.
Seat Rear Vertical Position | -- | Varies | This displays Volts. This is the voltage stored in memory for the seat rear vertical position.
Seat Recline Position | -- | Varies | This displays Volts. This is the voltage stored in memory for the seat recline position.

#### Memory Seat Module Scan Tool Output Controls

Scan Tool Output Control | Description
--- | ---
Clear Column Softstops | This output control is used to clear the steering column softstops stored in memory.
Front Up/Down | This output control is used to command the driver seat motor Up and Down.
Learn Column Softstops | This output control is used to program the steering column softstops.
Lumbar Forward/Rearward | This output control is used to command the driver seat lumbar forward and rearward.
Lumbar Up/Down | This output control is used to command the driver seat lumbar Up and Down.
Rear Up/Down | This output control is used to command the driver seat rear Up and Down.
Recline Forward/Rearward | This output control is used to command the driver seat reclining forward and rearward.
Seat Forward/Backward | This output control is used to command the driver seat forward and backward.
Telescope In/Out | This output control is used to command the telescope in and out.
Tilt Up/Down | This output control is used to command the tilt Up and Down.