For 1990-2009 cars

## Liftgate Trim Panel Replacement Enclave

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the liftgate window garnish molding. Refer to Liftgate Garnish Molding Replacement.

1 | Liftgate Trim Finish Panel Push Pin Retainer (Qty: 2)
2 | Liftgate Trim Finish Panel Assembly

#### Procedure

1. Use a trim panel removal tool to aid in the removal of the trim panel from the liftgate assembly.
2. Disconnect the electrical connector, if equipped.

3 | Liftgate Trim Finish Panel Retainer (Qty: 6)
4 | Liftgate Trim Finish Panel Clips (Qty: 2)

## Liftgate Trim Panel Replacement Traverse

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the liftgate window garnish molding. Refer to Liftgate Garnish Molding Replacement.

1 | Liftgate Inside Pull Handle Cover
2 | Liftgate Trim Finish Panel Screw (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 2 N·m (18 lb in)
3 | Liftgate Trim Finish Panel Push Pin Retainer (Qty: 2)
4 | Liftgate Trim Finish Panel Retainer (Qty: 6)
5 | Liftgate Trim Finish Panel Assembly

#### Procedure

1. Use a trim panel removal tool to aid in the removal of the trim panel from the liftgate assembly.
2. Disconnect the electrical connector, if equipped.

## Liftgate Trim Panel Replacement Acadia or OUTLOOK

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the liftgate window garnish molding. Refer to Liftgate Garnish Molding Replacement.

1 | Liftgate Inside Pull Handle Cover
2 | Liftgate Trim Finish Panel Screw (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 2 N·m (18 lb in)
3 | Liftgate Trim Finish Panel Push Pin Retainer (Qty: 2)
4 | Liftgate Trim Finish Panel Retainer (Qty: 6)
5 | Liftgate Trim Finish Panel Assembly

#### Procedure

1. Use a trim panel removal tool to aid in the removal of the trim panel from the liftgate assembly.
2. Disconnect the electrical connector, if equipped.