For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Drain the transmission, refill when repair is completed. Refer to Transmission Fluid Replacement.
3. Remove the left transmission mount bracket. Refer to Transmission Mount Bracket Replacement - Left Side.

1 | Input Speed Sensor Bolt M6 x 25 Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

Apply threadlocker GM P/N 12345382 (Canadian P/N 10953489) or equivalent to the input speed sensor bolt.

Tighten
9 N·m (80 lb in)

2 | Input Speed Sensor (ISS)

#### Procedure

Pull the ISS out of the case cover just far enough to gain access to the ISS seal.

3 | Input Speed Sensor Seal

#### Procedure

• | Remove the ISS seal by pulling it over the end of the ISS base.

• | Install the new ISS Seal by gently stretching it over the ISS base. Overstretching the seal will cause it to not seal properly. The seal is coated with a dry lubricant. If the coating is missing, lubricate the seal with automatic transmission fluid prior to installation.