For 1990-2009 cars

## Body Side Emblem/Nameplate Replacement OUTLOOK

Callout | Component Name
--- | ---
1 | C Pillar Nameplate

1. Use a J 25070 or equivalent to remove the old nameplate. Clean all adhesive from the bodyside, wipe surface dry with a clean lint-free towel prior to installing new nameplate.
2. When removing protective liners from adhesive tape, be careful not to touch tape with hands and do not allow tape to come in contact with dirt or any foreign matter prior to adhesion.
3. Ensure full adhesion of the nameplate to the bodyside is made.

## Body Side Emblem/Nameplate Replacement Acadia

Callout | Component Name
--- | ---
1 | C Pillar Emblem / Nameplate Caution: Refer to Exterior Trim Emblem Removal Caution in the Preface section.

#### Procedure

1. Use a J 25070 or equivalent to remove the old emblem/nameplate. Clean all adhesive from the bodyside, wipe surface dry with a clean lint-free towel prior to installing new emblem/nameplate.
2. When removing protective liners from adhesive tape, be careful not to touch tape with hands and do not allow tape to come in contact with dirt or any foreign matter prior to adhesion.
3. Ensure full adhesion of the nameplate to the bodyside is made.