For 1990-2009 cars

## Quarter Lower Rear Trim Panel Replacement Traverse with TB5

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Move the rear seat to the full forward position.
2. Remove the rear number 2 seat. Refer to Rear Number 2 Seat Replacement.
3. Remove the rear quarter upper trim panel. Refer to Quarter Upper Trim Panel Replacement.
4. Disconnect the liftgate actuator rod from the liftgate. Refer to Liftgate Actuator Rod Replacement.
5. Disconnect the rear seat number 2 shoulder belt anchor bolt. Refer to Rear Seat Number 2 Retractor Side Belt Replacement.

1 | Cargo Tie Down Loop Bolt Cap (Qty: 2)
2 | Cargo Tie Down Loop Bolt (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 3 N·m (27 lb in)
3 | Cargo Tie Down Loop (Qty: 2)
4 | Body Side Trim Panel Armrest Tip Pull upward on the armrest to disengage the retainer clips.
5 | Cargo Screen Retainer Assembly Tip Twist and pull outward to remove the retainer.
6 | Rear Quarter Lower Trim Panel Bolt (Qty: 2) Tighten 3 N·m (27 lb in)
7 | Rear Quarter Lower Trim Panel Assembly

#### Procedure

1. Pull outward to disengage the trim panel retainers.
2. Disconnect the electrical connectors.

## Quarter Lower Rear Trim Panel Replacement Traverse without TB4

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Move the rear seat to the full forward position.
2. Remove the rear number 2 seat. Refer to Rear Number 2 Seat Replacement.
3. Remove the rear quarter upper trim panel. Refer to Quarter Upper Trim Panel Replacement.
4. Disconnect the liftgate actuator rod from the liftgate. Refer to Liftgate Actuator Rod Replacement.
5. Disconnect the rear seat number 2 shoulder belt anchor bolt. Refer to Rear Seat Number 2 Retractor Side Belt Replacement.

1 | Cargo Tie Down Loop Bolt Cap (Qty: 2)
2 | Cargo Tie Down Loop Bolt (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 3 N·m (27 lb in)
3 | Cargo Tie Down Loop (Qty: 2)
4 | Body Side Trim Panel Armrest Tip Pull upward on the armrest to disengage the retainer clips.
5 | Cargo Screen Retainer Assembly Tip Twist and pull outward to remove the retainer.
6 | Rear Quarter Lower Trim Panel Bolt (Qty: 2) Tighten 3 N·m (27 lb in)
7 | Rear Quarter Lower Trim Panel Assembly

#### Procedure

1. Pull outward to disengage the trim panel retainers.
2. Disconnect the electrical connectors.

## Quarter Lower Rear Trim Panel Replacement Acadia/OUTLOOKwith TB5

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Move the rear seat to the full forward position.
2. Remove the rear number 2 seat. Refer to Rear Number 2 Seat Replacement.
3. Remove the rear quarter upper trim panel. Refer to Quarter Upper Trim Panel Replacement.
4. Disconnect the liftgate actuator rod from the liftgate. Refer to Liftgate Actuator Rod Replacement.
5. Disconnect the rear seat number 2 shoulder belt anchor bolt. Refer to Rear Seat Number 2 Retractor Side Belt Replacement.

1 | Cargo Tie Down Loop Bolt Cap (Qty: 2)
2 | Cargo Tie Down Loop Bolt (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 3 N·m (27 lb in)
3 | Cargo Tie Down Loop (Qty: 2)
4 | Body Side Trim Panel Armrest Tip Pull upward on the armrest to disengage the retainer clips.
5 | Cargo Screen Retainer Assembly Tip Twist and pull outward to remove the retainer.
6 | Rear Quarter Lower Trim Panel Bolt (Qty: 2) Tighten 3 N·m (27 lb in)
7 | Rear Quarter Lower Trim Panel Assembly

#### Procedure

1. Pull outward to disengage the trim panel retainers.
2. Disconnect the electrical connectors.

## Quarter Lower Rear Trim Panel Replacement Acadia/OUTLOOK without TB4

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Move the rear seat to the full forward position.
2. Remove the rear number 2 seat. Refer to Rear Number 2 Seat Replacement.
3. Remove the rear quarter upper trim panel. Refer to Quarter Upper Trim Panel Replacement.
4. Disconnect the liftgate actuator rod from the liftgate. Refer to Liftgate Actuator Rod Replacement.
5. Disconnect the rear seat number 2 shoulder belt anchor bolt. Refer to Rear Seat Number 2 Retractor Side Belt Replacement.

1 | Cargo Tie Down Loop Bolt Cap (Qty: 2)
2 | Cargo Tie Down Loop Bolt (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 3 N·m (27 lb in)
3 | Cargo Tie Down Loop (Qty: 2)
4 | Body Side Trim Panel Armrest Tip Pull upward on the armrest to disengage the retainer clips.
5 | Cargo Screen Retainer Assembly Tip Twist and pull outward to remove the retainer.
6 | Rear Quarter Lower Trim Panel Bolt (Qty: 2) Tighten 3 N·m (27 lb in)
7 | Rear Quarter Lower Trim Panel Assembly

#### Procedure

1. Pull outward to disengage the trim panel retainers.
2. Disconnect the electrical connectors.

## Quarter Lower Rear Trim Panel Replacement Enclave with TB5

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Move the rear seat to the full forward position.
2. Remove the rear number 2 seat. Refer to Rear Number 2 Seat Replacement.
3. Remove the rear quarter upper trim panel. Refer to Quarter Upper Trim Panel Replacement.
4. Disconnect the liftgate actuator rod from the liftgate. Refer to Liftgate Actuator Rod Replacement.
5. Disconnect the rear seat number 2 shoulder belt anchor bolt. Refer to Rear Seat Number 2 Retractor Side Belt Replacement.

1 | Cargo Tie Down Loop Bolt Cap (Qty: 2)
2 | Cargo Tie Down Loop Bolt (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 3 N·m (27 lb in)
3 | Cargo Tie Down Loop (Qty: 2)
4 | Body Side Trim Panel Armrest Tip Pull upward on the armrest to disengage the retainer clips.
5 | Cargo Screen Retainer Assembly Tip Twist and pull outward to remove the retainer.
6 | Rear Quarter Lower Trim Panel Bolt (Qty: 2) Tighten 3 N·m (27 lb in)
7 | Rear Quarter Lower Trim Panel Assembly

#### Procedure

1. Pull outward to disengage the trim panel retainers.
2. Disconnect the electrical connectors.
3. Transfer components as necessary.

## Quarter Lower Rear Trim Panel Replacement Enclave without TB4

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Move the rear seat to the full forward position.
2. Remove the rear number 2 seat. Refer to Rear Number 2 Seat Replacement.
3. Remove the rear quarter upper trim panel. Refer to Quarter Upper Trim Panel Replacement.
4. Disconnect the liftgate actuator rod from the liftgate. Refer to Liftgate Actuator Rod Replacement.
5. Disconnect the rear seat number 2 shoulder belt anchor bolt. Refer to Rear Seat Number 2 Retractor Side Belt Replacement.

1 | Cargo Tie Down Loop Bolt Cap (Qty: 2)
2 | Cargo Tie Down Loop Bolt (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 3 N·m (27 lb in)
3 | Cargo Tie Down Loop (Qty: 2)
4 | Body Side Trim Panel Armrest Tip Pull upward on the armrest to disengage the retainer clips.
5 | Cargo Screen Retainer Assembly Tip Twist and pull outward to remove the retainer.
6 | Rear Quarter Lower Trim Panel Bolt (Qty: 2) Tighten 3 N·m (27 lb in)
7 | Rear Quarter Lower Trim Panel Assembly

#### Procedure

1. Pull outward to disengage the trim panel retainers.
2. Disconnect the electrical connectors.
3. Transfer components as necessary.