For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the evaporative emission (EVAP) canister. Refer to Evaporative Emission Canister Replacement.

1 | Evaporative Emission Canister
2 | Evaporative Emission Canister Vent Solenoid Valve Hose

#### Procedure

1. Disconnect the quick connect fitting at the EVAP canister. Refer to Plastic Collar Quick Connect Fitting Service.
2. Push in the retainer on the rear of the EVAP canister disengaging the vent solenoid valve.