For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Set the park brake and chock the wheels.
2. Remove the air cleaner assembly. Refer to Air Cleaner Assembly Replacement.

1 | Transmission Range Selector Lever Cable
2 | Transmission Range Selector Lever Cable Bracket Bolt Caution: Refer to Fastener Caution in the Preface section. Tighten 25 N·m (18 lb ft)
3 | Transmission Range Selector Lever Cable Bracket