For 1990-2009 cars

## Rear Seat Head Restraint Replacement with 40 Percent Seat

Callout | Component Name
--- | ---
1 | Rear Seat Head Restraint

#### Procedure

1. Push down on the seat back cover at the base of the head restraint to access the clips on the head restraint guides.
2. Remove the head restraint guide clips to release the head restraint.
3. Slide the head restraint up to remove.

## Rear Seat Head Restraint Replacement with 60 Percent Seat

Callout | Component Name
--- | ---
1 | Rear Seat Head Restraint

#### Procedure

1. Push down on the seat back cover at the base of the head restraint to access the clips on the head restraint guides.
2. Remove the head restraint guide clips to release the head restraint.
3. Slide the head restraint up to remove.