For 1990-2009 cars

## Driver Knee Bolster Replacement Traverse

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the hood latch release handle assembly. Refer to Hood Primary Latch Release Cable Handle Replacement.

1 | Driver Knee Bolster Screw (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 2.5 N·m (22 lb in)
2 | Driver Knee Bolster Assembly

#### Procedures

1. Disconnect the electrical connections.
2. When replacing the knee bolster, transfer all necessary components.

## Driver Knee Bolster Replacement Acadia

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the hood latch release handle assembly. Refer to Hood Primary Latch Release Cable Handle Replacement.

1 | Driver Knee Bolster Screw (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 2.5 N·m (22 lb in)
2 | Drivers Knee Bolster Assembly

#### Procedure

1. Disconnect the electrical connections.
2. When replacing the drivers knee bolster, transfer all necessary components.

3 | Retainer Clip (Qty: 5)

## Driver Knee Bolster Replacement Enclave

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the hood latch release handle assembly. Refer to Hood Primary Latch Release Cable Handle Replacement.

1 | Driver Knee Bolster Screw (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 2.5 N·m (22 lb in)
2 | Driver Knee Bolster Assembly

#### Procedures

1. Disconnect the electrical connections.
2. When replacing the knee bolster, transfer all necessary components.

3 | Retainer Clip (Qty: 5)

## Driver Knee Bolster Replacement OUTLOOK

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the hood latch release handle assembly. Refer to Hood Primary Latch Release Cable Handle Replacement.

1 | Driver Knee Bolster Screw (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 2.5 N·m(22 in lb)
2 | Driver Knee Bolster Assembly

#### Procedure

1. Disconnect the electrical connections.
2. When replacing the steering column opening filler, transfer all necessary components.

3 | Retainer Clip (Qty: 5)