For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Bolt Access Plug Tip Use a plastic flat-bladed tool to remove.
2 | Front Side Door Outside Handle Bolt Caution: Refer to Fastener Caution in the Preface section. Tighten 9 N·m (80 lb in)
3 | Front Door Outside Handle Cap
4 | Front Door Outside Handle Cap Gasket
5 | Front Door Outside Handle Tip Pull the outside handle rearward to release it from the inside handle housing.
6 | Front Door Outside Handle Gasket