For 1990-2009 cars

## Rear Seat Cushion Trim Panel Assembly Replacement - Inboard with 40 Percent Seat

Callout | Component Name
--- | ---
1 | Rear Seat Cushion Trim Panel Assembly

#### Procedure

Remove the trim panel by pulling the front edge outward and then sliding the trim panel rearward to release from the seat.

## Rear Seat Cushion Trim Panel Assembly Replacement - Inboard with 60 Percent Seat

Callout | Component Name
--- | ---
1 | Rear Seat Cushion Trim Panel Assembly

#### Procedure

Remove the trim panel by pulling the front edge outward and then sliding the trim panel rearward to release from the seat.