For 1990-2009 cars

## Headlamp Bulb Replacement OUTLOOK TVD and T96

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the headlamp assembly. Refer to Headlamp Replacement.

1 | Headlamp Bulb Accessory Cover Tip Rotate the cover counter-clockwise and remove.
2 | Headlamp Bulb

#### Procedure

Release the wire clip from the bulb and disconnect the electrical connector in order to remove the bulb from the lamp assembly.

## Headlamp Bulb Replacement Traverse without TVP High Beam

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the headlamp assembly. Refer to Headlamp Replacement.

1 | Headlamp Bulb Accessory Cover Tip Rotate counterclockwise and remove.
2 | High Beam Bulb Warning: Refer to Halogen Bulb Warning in the Preface section. Tip Disconnect the electrical connector in order to remove the bulb.

## Headlamp Bulb Replacement Traverse with TVP Lo Beam

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the headlamp assembly. Refer to Headlamp Replacement.

1 | Headlamp Bulb Accessory Cover Tip Rotate counterclockwise and remove.
2 | Low Beam / DRL Bulb Warning: Refer to Halogen Bulb Warning in the Preface section. Tip Disconnect the electrical connector in order to remove the low beam / DRL bulb.

## Headlamp Bulb Replacement Traverse without TVP Lo Beam

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the headlamp assembly. Refer to Headlamp Replacement.

1 | Headlamp Bulb Accessory Cover Tip Rotate counterclockwise and remove.
2 | Low Beam Bulb Warning: Refer to Halogen Bulb Warning in the Preface section. Tip Disconnect the electrical connector in order to remove the low beam bulb socket.

## Headlamp Bulb Replacement High Beam without T96

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the front wheelhouse liner. Refer to Front Wheelhouse Front Liner Replacement.

1 | Headlamp Bulb Accessory Cover Tip Rotate the cover counterclockwise and remove.
2 | Headlamp Bulb (High Beam) Warning: Refer to Halogen Bulb Warning in the Preface section.

#### Procedure

1. Disconnect the electrical connector from the bulb socket.
2. Disconnect the bulb socket from the headlamp assembly.
3. Discard the bulb.

## Headlamp Bulb Replacement Low Beam without T96

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the front wheelhouse liner. Refer to Front Wheelhouse Front Liner Replacement.

1 | Headlamp Bulb Accessory Cover Tip Rotate the cover counterclockwise and remove.
2 | Headlamp Bulb (Low Beam) Warning: Refer to Halogen Bulb Warning in the Preface section.

#### Procedure

1. Disconnect the electrical connector from the bulb socket.
2. Release the bulb from the headlamp assembly.
3. Discard the bulb.

## Headlamp Bulb Replacement OUTLOOK Non HID

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the headlamp assembly. Refer to Headlamp Replacement.

1 | Headlamp Bulb Accessory Covers (Qty: 2)
2 | Headlamp Bulb Assembly (High Beam) Warning: Refer to Halogen Bulb Warning in the Preface section. Tip Disconnect the electrical connectors and remove the bulbs.
3 | Headlamp Bulb Assembly (Low Beam)