For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the instrument panel insulator - right side. Refer to Instrument Panel Insulator Panel Replacement - Right Side.

1 | Blower Motor Screw Caution: Refer to Fastener Caution in the Preface section. Tighten 2 N·m (18 lb in)
2 | Blower Motor

#### Procedure

• | Disconnect the electrical connectors.

• | Rotate the blower motor counterclockwise to remove.