For 1990-2009 cars

Callout | Component Name
--- | ---
Caution: In order to avoid actuator damage, DO NOT apply power to the actuator when it is not installed in the HVAC module.

#### Preliminary Procedure

Remove the instrument panel insulator - left side. Refer to Instrument Panel Insulator Panel Replacement - Left Side.

1 | Left Temperature Actuator Screw (Qty: 3) Caution: Refer to Fastener Caution in the Preface section. Tighten 2 N·m (18 lb in)
2 | Left Temperature Actuator

#### Procedure

1. Disconnect the electrical connectors.
2. Re-calibrate the right temperature actuator. Refer to Actuator Recalibration.