For 1990-2009 cars

## Liftgate Emblem/Nameplate Replacement TRAVERSE AWD

Callout | Component Name
--- | ---
1 | Liftgate Nameplate Assembly Caution: Refer to Exterior Trim Emblem Removal Caution in the Preface section.

#### Procedure

1. The part and surface should be 21°C (70°F) prior to installation. The vehicle should remain 21°C (70°F) for one hour after assembly to allow adhesive to develop sufficient bond strength.
2. Use a J 25070 Heat Gun or equivalent to remove the old emblem. Clean all adhesive from rear liftgate and wipe the surface dry with a clean lint-free towel prior to installing the new emblem / nameplate.
3. Close the liftgate.
4. When removing protective liners from the adhesive tape, be careful not to touch tape with hands and do not allow tape to come in contact with dirt or any foreign matter prior to adhesion.
5. Apply the liftgate nameplate to the desired location on the liftgate.
6. Wet out the emblem and ensure full adhesion of the emblem to the liftgate is made.

## Liftgate Emblem/Nameplate Replacement TRAVERSE LS LT LTZ

Callout | Component Name
--- | ---
1 | Liftgate Trim Nameplate Assembly (LS LT LTZ) Caution: Refer to Exterior Trim Emblem Removal Caution in the Preface section.

#### Procedure

1. Use a J 25070 or equivalent to remove the old nameplate. Clean all the adhesive residue from the liftgate, wipe the surface dry with a clean lint-free towel prior to installing new nameplate.
2. When removing protective liners from adhesive backed nameplates, be careful not to touch the tape with hands and do not allow the tape to come in contact with dirt or any foreign matter prior to adhesion.
3. Close the liftgate prior to installing the new nameplate/emblem to the liftgate.
4. Remove the protective liner from the back side of the adhesive tape.
5. Position the nameplate/emblem to the liftgate and press to ensure full adhesion is made.

## Liftgate Emblem/Nameplate Replacement Chevrolet

Callout | Component Name
--- | ---
1 | Liftgate Nameplate Assembly Caution: Refer to Exterior Trim Emblem Removal Caution in the Preface section.

#### Procedure

1. The part and surface should be 21°C (70°F) prior to installation. The vehicle should remain 21°C (70°F) for one hour after assembly to allow adhesive to develop sufficient bond strength.
2. Use a J 25070 Heat Gun or equivalent to remove the old emblem. Clean all adhesive from rear liftgate and wipe the surface dry with a clean lint-free towel prior to installing the new emblem / nameplate.
3. Close the liftgate.
4. When removing protective liners from the adhesive tape, be careful not to touch tape with hands and do not allow tape to come in contact with dirt or any foreign matter prior to adhesion.
5. Apply the liftgate nameplate to the desired location on the liftgate.
6. Wet out the emblem and ensure full adhesion of the emblem to the liftgate is made.

## Liftgate Emblem/Nameplate Replacement Acadia

Callout | Component Name
--- | ---
1 | Liftgate Nameplate/Emblem Caution: Refer to Exterior Trim Emblem Removal Caution in the Preface section.

#### Procedure

1. Use a J 25070 or equivalent to remove the old nameplate. Clean all the adhesive residue from the liftgate, wipe the surface dry with a clean lint-free towel prior to installing new nameplate.
2. When removing protective liners from adhesive backed nameplates, be careful not to touch the tape with hands and do not allow the tape to come in contact with dirt or any foreign matter prior to adhesion.
3. Close the liftgate prior to installing the new nameplate/emblem to the liftgate.
4. Remove the protective liner from the back side of the adhesive tape.
5. Align the nameplate/emblem to the liftgate and press to ensure full adhesion is made.

## Liftgate Emblem/Nameplate Replacement AWD Acadia

Callout | Component Name
--- | ---
1 | Liftgate Nameplate/Emblem Caution: Refer to Exterior Trim Emblem Removal Caution in the Preface section.

#### Procedure

1. Use a J 25070 or equivalent to remove the old nameplate. Clean all the adhesive residue from the liftgate, wipe the surface dry with a clean lint-free towel prior to installing new nameplate.
2. When removing protective liners from adhesive backed nameplates, be careful not to touch the tape with hands and do not allow the tape to come in contact with dirt or any foreign matter prior to adhesion.
3. Close the liftgate prior to installing the new nameplate/emblem to the liftgate.
4. Remove the protective liner from the back side of the adhesive tape.
5. Align the nameplate/emblem to the liftgate and press to ensure full adhesion is made.

## Liftgate Emblem/Nameplate Replacement Enclave Nameplate

Callout | Component Name
--- | ---
1 | Liftgate Emblem (ENCLAVE) Caution: Refer to Exterior Trim Emblem Removal Caution in the Preface section.

#### Procedure

1. Use a J 25070 or equivalent to remove the old emblem. Clean all the adhesive residue from the liftgate, wipe the surface dry with a clean lint-free towel prior to installing new emblem.
2. When removing protective liners from adhesive backed emblems, be careful not to touch the tape with hands and do not allow the tape to come in contact with dirt or any foreign matter prior to adhesion.
3. Close the liftgate prior to installing the new emblem to the liftgate.
4. Remove the protective liner from the back side of the adhesive tape.
5. Align the emblem to the liftgate and press to ensure full adhesion is made.

2 | Liftgate Emblem (CX, CXL)

#### Procedure

1. Use a J 25070 or equivalent to remove the old emblem. Clean all the adhesive residue from the endgate, wipe the surface dry with a clean lint-free towel prior to installing new emblem.
2. When removing protective liners from adhesive backed emblems, be careful not to touch the tape with hands and do not allow the tape to come in contact with dirt or any foreign matter prior to adhesion.
3. Close the liftgate prior to installing the new emblem to the liftgate.
4. Remove the protective liner from the back side of the adhesive tape.
5. Align the emblem to the liftgate and press to ensure full adhesion is made.

3 | Liftgate Nameplate (BUICK)

#### Procedure

1. Use a J 25070 or equivalent to remove the old nameplate. Clean all the adhesive residue from the liftgate, wipe the surface dry with a clean lint-free towel prior to installing new nameplate.
2. When removing protective liners from adhesive backed nameplates, be careful not to touch the tape with hands and do not allow the tape to come in contact with dirt or any foreign matter prior to adhesion.
3. Close the liftgate prior to installing the new nameplate to the liftgate.
4. Remove the protective liner from the back side of the adhesive tape.
5. Align the nameplate to the liftgate and press to ensure full adhesion is made.

## Liftgate Emblem/Nameplate Replacement Enclave Tri Shield

Callout | Component Name
--- | ---
1 | Liftgate Emblem (Tri-Shield) Caution: Refer to Exterior Trim Emblem Removal Caution in the Preface section.

#### Procedure

1. Use a J 25070 or equivalent to remove the old emblem. Clean all the adhesive residue from the liftgate, wipe the surface dry with a clean lint-free towel prior to installing new emblem.
2. When removing protective liners from adhesive backed emblems, be careful not to touch the tape with hands and do not allow the tape to come in contact with dirt or any foreign matter prior to adhesion.
3. Close the liftgate prior to installing the new emblem to the liftgate.
4. Remove the protective liner from the back side of the adhesive tape.
5. Align the emblem to the two guide holes in the liftgate outer panel and press to ensure full adhesion is made.

## Liftgate Emblem/Nameplate Replacement OUTLOOK

Callout | Component Name
--- | ---
1 | OUTLOOK Emblem / Nameplate Caution: Refer to Exterior Trim Emblem Removal Caution in the Preface section.

#### Procedure

1. The part and surface should be 21°C (70°F) prior to installation. The vehicle should remain 21°C (70°F) for one hour after assembly to allow adhesive to develop sufficient bond strength.
2. Use a J 25070 Heat Gun or equivalent to remove the old emblem. Clean all adhesive from rear liftgate and wipe the surface dry with a clean lint-free towel prior to installing the new emblem / nameplate.
3. When removing protective liners from the adhesive tape, be careful not to touch tape with hands and do not allow tape to come in contact with dirt or any foreign matter prior to adhesion.
4. Close the liftgate.
5. Wet out the emblem and ensure full adhesion of the emblem to the liftgate is made.

## Liftgate Emblem/Nameplate Replacement OUTLOOK AWD

Callout | Component Name
--- | ---
1 | Outlook Emblem / Nameplate Caution: Refer to Exterior Trim Emblem Removal Caution in the Preface section.

#### Procedure

1. The part and surface should be 21°C (70°F) prior to installation. The vehicle should remain 21°C (70°F) for one hour after assembly to allow adhesive to develop sufficient bond strength.
2. Use a J 25070 Heat Gun or equivalent to remove the old emblem. Clean all adhesive from rear liftgate and wipe the surface dry with a clean lint-free towel prior to installing the new emblem / nameplate.
3. When removing protective liners from the adhesive tape, be careful not to touch tape with hands and do not allow tape to come in contact with dirt or any foreign matter prior to adhesion.
4. Close the liftgate.
5. Wet out the emblem and ensure full adhesion of the emblem to the liftgate is made.

## Liftgate Emblem/Nameplate Replacement OUTLOOK XR

Callout | Component Name
--- | ---
1 | OUTLOOK Emblem / Nameplate Caution: Refer to Exterior Trim Emblem Removal Caution in the Preface section.

#### Procedure

1. The part and surface should be 21°C (70°F) prior to installation. The vehicle should remain 21°C (70°F) for one hour after assembly to allow adhesive to develop sufficient bond strength.
2. Use a J 25070 Heat Gun or equivalent to remove the old emblem. Clean all adhesive from rear liftgate and wipe the surface dry with a clean lint-free towel prior to installing the new emblem / nameplate.
3. When removing protective liners from the adhesive tape, be careful not to touch tape with hands and do not allow tape to come in contact with dirt or any foreign matter prior to adhesion.
4. Close the liftgate.
5. Wet out the emblem and ensure full adhesion of the emblem to the liftgate is made.