For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the right engine strut mount. Refer to Engine Mount Strut Replacement - Right Side.
2. Remove the right engine mount strut bracket. Refer to Engine Mount Strut Bracket Replacement - Right Side.
3. Remove the drive belt. Refer to Drive Belt Replacement.

1 | Idler Pulley Bolt Caution: Refer to Fastener Caution in the Preface section. Tighten 50 N·m (37 lb ft)
2 | Tensioner Bolt Tighten 50 N·m (37 lb ft)
3 | Tensioner Tip Remove wire harness retainer from tensioner.